Next: Score Options, Previous: RS/6000 and PowerPC Options, Up: Submodel Options

#### 3.17.28 S/390 and zSeries Options

These are the -m options defined for the S/390 and zSeries architecture.

`-mhard-float`
`-msoft-float`
  Use (do not use) the hardware floating-point instructions and registers for floating-point operations. When -msoft-float is specified, functions in libgcc.a will be used to perform floating-point operations. When -mhard-float is specified, the compiler generates IEEE floating-point instructions. This is the default.
`-mlong-double-64`
`-mlong-double-128`
  These switches control the size of `long double` type. A size of 64bit makes the `long double` type equivalent to the `double` type. This is the default.
`-mbackchain`
`-mno-backchain`
  Store (do not store) the address of the caller's frame as backchain pointer into the callee's stack frame. A backchain may be needed to allow debugging using tools that do not understand DWARF-2 call frame information. When -mno-packed-stack is in effect, the backchain pointer is stored at the bottom of the stack frame; when -mpacked-stack is in effect, the backchain is placed into the topmost word of the 96/160 byte register save area.

  In general, code compiled with -mbackchain is call-compatible with code compiled with -mmo-backchain; however, use of the backchain for debugging purposes usually requires that the whole binary is built with -mbackchain. Note that the combination of -mbackchain, -mpacked-stack and -mhard-float is not supported. In order to build a linux kernel use -msoft-float.

  The default is to not maintain the backchain.

`-mpacked-stack`
`-mno-packed-stack`
  Use (do not use) the packed stack layout. When -mno-packed-stack is specified, the compiler uses the all fields of the 96/160 byte register save area only for their default purpose; unused fields still take up stack space. When -mpacked-stack is specified, register save slots are densely packed at the top of the register save area; unused space is reused for other purposes, allowing for more efficient use of the available stack space. However, when -mbackchain is also in effect, the topmost word of the save area is always used to store the backchain, and the return address register is always saved two words below the backchain.

  As long as the stack frame backchain is not used, code generated with -mpacked-stack is call-compatible with code generated with -mno-packed-stack. Note that some non-FSF releases of GCC 2.95 for S/390 or zSeries generated code that uses the stack frame backchain at run time, not just for debugging purposes. Such code is not call-compatible with code compiled with -mpacked-stack. Also, note that the combination of -mbackchain, -mpacked-stack and -mhard-float is not supported. In order to build a linux kernel use -msoft-float.

  The default is to not use the packed stack layout.

`-msmall-exec`
`-mno-small-exec`
  Generate (or do not generate) code using the `bras` instruction to do subroutine calls. This only works reliably if the total executable size does not exceed 64k. The default is to use the `basr` instruction instead, which does not have this limitation.
`-m64`
`-m31`
  When -m31 is specified, generate code compliant to the GNU/Linux for S/390 ABI. When -m64 is specified, generate code compliant to the GNU/Linux for zSeries ABI. This allows GCC in particular to generate 64-bit instructions. For the s390 targets, the default is -m31, while the s390x targets default to -m64.
`-mzarch`
`-mesa`
  When -mzarch is specified, generate code using the instructions available on z/Architecture. When -mesa is specified, generate code using the instructions available on ESA/390. Note that -mesa is not possible with -m64. When generating code compliant to the GNU/Linux for S/390 ABI, the default is -mesa. When generating code compliant to the GNU/Linux for zSeries ABI, the default is -mzarch.
`-mmvcle`
`-mno-mvcle`
  Generate (or do not generate) code using the `mvcle` instruction to perform block moves. When -mno-mvcle is specified, use a `mvc` loop instead. This is the default unless optimizing for size.
`-mdebug`
`-mno-debug`
  Print (or do not print) additional debug information when compiling. The default is to not print debug information.
`-march=`cpu-type
  Generate code that will run on cpu-type, which is the name of a system representing a certain processor type. Possible values for cpu-type are g5, g6, z900, and z990. When generating code using the instructions available on z/Architecture, the default is -march=z900. Otherwise, the default is -march=g5.
`-mtune=`cpu-type
  Tune to cpu-type everything applicable about the generated code, except for the ABI and the set of available instructions. The list of cpu-type values is the same as for -march. The default is the value used for -march.
`-mtpf-trace`
`-mno-tpf-trace`
  Generate code that adds (does not add) in TPF OS specific branches to trace routines in the operating system. This option is off by default, even when compiling for the TPF OS.
`-mfused-madd`
`-mno-fused-madd`
  Generate code that uses (does not use) the floating point multiply and accumulate instructions. These instructions are generated by default if hardware floating point is used.
`-mwarn-framesize=`framesize
  Emit a warning if the current function exceeds the given frame size. Because this is a compile time check it doesn't need to be a real problem when the program runs. It is intended to identify functions which most probably cause a stack overflow. It is useful to be used in an environment with limited stack size e.g. the linux kernel.
`-mwarn-dynamicstack`
  Emit a warning if the function calls alloca or uses dynamically sized arrays. This is generally a bad idea with a limited stack size.
`-mstack-guard=`stack-guard
`-mstack-size=`stack-size
  If these options are provided the s390 back end emits additional instructions in the function prologue which trigger a trap if the stack size is stack-guard bytes above the stack-size (remember that the stack on s390 grows downward). If the stack-guard option is omitted the smallest power of 2 larger than the frame size of the compiled function is chosen. These options are intended to be used to help debugging stack overflow problems. The additionally emitted code causes only little overhead and hence can also be used in production like systems without greater performance degradation. The given values have to be exact powers of 2 and stack-size has to be greater than stack-guard without exceeding 64k. In order to be efficient the extra code makes the assumption that the stack starts at an address aligned to the value given by stack-size. The stack-guard option can only be used in conjunction with stack-size.